KSFDC

**Location Recording Equipments**

|  |  |  |
| --- | --- | --- |
| Serial No | Description of Items | Quantity |
|  | **Documentary/Advertisement /Ambience**  |  |
| 1 | Sound Device 633 Six-Input Compact Mixer With 10-Track Recorder & Auto mixing | 1 |
| 2 | Sennenheisser MKH 416-P48U3-Short shotgun interference tube microphone. | 1 |
| 3 | Sennenheisser MKH 416/60-P48U3-Short shotgun interference tube microphone- Blimp Kit | 2 |
| 4 | [Lectrosonics LMb Digital Hybrid Wireless Belt pack Transmitter (B1: 537.600 to 614.375 MHz)](https://www.bhphotovideo.com/c/product/1048158-REG/lectrosonics_lmb_b1_lmb_belt_pack_transmit.html) | 3 |
| 5 | Lectrosonics L Series LR Mini Hybrid Portable Wireless Receiver (B1: 537.600 to 614.375 MHz) withTA3F to XLRM CableTA3F to 1/8" TRS CableCamera Shoe Mount AdapterZippered Carrying Pouch | 3 |
| 6 | Sanken COS-11D Omni Lavalier Mic, Normal Sens, Hardwired TA5F Connector for LectrosonicsTransmitter (with Accessories, 3Black+2white) | 5 |
| 7 | SAM 32 CF card 32 GB | 2 |
| 8 | SAM 32 SDXC/SDHC card 32 GB | 2 |
| 9 | ORCA OR-34 Audio / Mixer Bag for 633 | 1 |
| 10 | Sennheiserew 112P G4 Camera-Mount Wireless Microphone System(Transmitter and Receiver ) with ME 2-II Lavalier Mic A: (516 to 558 MHz) for camera Pilotwith Output cable, Bag and accessories | 1 |
| 11 | K-Tek K-152 5-Section Klassic Series Lightweight Boompole 12 feet | 1 |
| 12 | K-Tek K-202CCR 5-Section Graphite Fiber Boom Pole 16 feet | 1 |
| 13 | Sony NP-F970 L-series Info-Lithium Battery (7.2v, 6300mAh) | 3 |
| 14 | Sony AC Adapter and Twin Charger For L-Series Batteries | 1 |
| 15 | Sony MDR-7506 Headphone | 1 |
| 16 | Transcend RDF8 USB 3.1 Gen 1 Card Reader | 3 |
| 17 | Sennheiser HD 206 507364 Headphone (for Director) | 1 |
| 18 | Snnenheisser MKH 60-1 Lightweight short gun microphone with Cardioid Polar Pattern  | 1 |
| 19 | Sennenheisser MKH30-P48 RF condenser microphone with figure-of-eight pick-up pattern | 1 |
| 20 | Rycote Stereo Cyclone MS Kit 12 Windshield System for Sennheiser MKH 30 and MKH 60 | 1 |
| 21 | 5-Pin Stereo XLR Female to Dual XLR Male Y-Cable not less than six meter  | 1 |
|  | **Cables and Accessories etc** |  |